|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|

|  |
| --- |
| press release |
| page 1 of 1 |
|  |
| Forbo’s Flame-Retardant Belts Excel on Curved Conveyors |

 |

[lead]

Hanover, December 9, 2021 – New Curved Belt for Conveying Baggage and Parcels

[Body]

The key criterion for curved belts is an even distribution of force in the fabric in all directions (lengthways, crossways and diagonally) to ensure the belt tracks without any creases and bulges. The belt has to be made of exceptionally tear-resistant fabric because in many applications the profiles sewn on to the outside radius need to absorb all the force. As a result, Forbo Movement Systems developed the new E 12/2 0/V6 MT-C-SE black (art. no. 906882) Transilon belt for two well-known OEMs in Germany and Austria. The belt has already been successfully deployed for conveying baggage at airports and parcels in fulfilment centers. This conveyor belt is flame retardant (SE), has a matte surface pattern and can be used on all curved conveyors belonging to other OEMs. The exceptional accumulation functionality rounds out its exceptional profile of characteristics.

For further information:

Matthias Eilert

Marketing Communications

Phone +49 511 67 04 232

siegling@forbo.com